To start PanVIEW;

Open an xterm window

cd my\_cosmos

source setup\_SISPI

start\_panapp\_des \_acq12 (slot 6)

To start dashboard

Open an xterm window

cd my\_cosmos

source setup\_SISPI

cd ..

cd utils/dashboard

source setup\_dashboard

dashboard \_acq12

Port number for dashboard is 5425

Problem with slink try

pan close

pan init

Download firmware on 12ch board

Open xterm window

Source setup\_xilinx

cd firmware/acq12/Xilinx

make program

read the “other bits” on the dashboard 12ch test

firmware should = 0x198 (4.08)

focal planes live in my\_cosmos/panview\_des/fpas

Jamieson’s Attribute Editor

Open xterm window

Cd utils/jamieson

Python pae.py